ОРИГИНАЛ - RUS	ПЕРЕВОД - ENG	
 Ðàçáîðíàÿ ìåòàëëè÷åñêàÿ æåëîáîâàÿ ñèñòåìà ôàáðè÷íîãî èçãîòîâëåíèÿ â ðàçëè÷íûõ âàðèàíòàõ, ïðîèçâåäåííàÿ ïî ìåæäóíàðîäíîìó ñòàíäàðòó IEC 61537, ÿâëÿåòñÿ èäåàëüíûì ðåøåíèåì äëÿ ðàñïðåäåëåíèÿ, çàùèòû è çàêðåïëåíèÿ ýëåêòðè÷åñêèõ êàáåëåé â çäàíèÿõ ãðàæäàíñêîãî, îáñëóæèâàþùåãî è ïðîìûøëåííîãî íàçíà÷åíèÿ.
Ëåãêîñòü ïåðåõîäà îò îäíîãî ðàçìåðà ê äðóãîìó îáåñïå÷èâàåòñÿ ðàçíîîáðàçíûìè ñîåäèíèòåëüíûìè ýëåìåíòàìè, êîòîðûå ÿâëÿþòñÿ ñîñòàâíîé ÷àñòüþ øèðîêîãî ñïåêòðà âñïîìîãàòåëüíîãî îáîðóäîâàíèÿ, ïîçâîëÿþùåãî óñòàíàâëèâàòü ñèñòåìó äàæå íà èçâèëèñòûõ ó÷àñòêàõ ïî êðàò÷àéøåìó ïóòè è, ïðåæäå âñåãî, áåç íåîáõîäèìîñòè ïåðåîáîðóäîâàíèÿ.
Ìíîãèå ýëåìåíòû ñèñòåìû FEMI 3, â ÷àñòíîñòè ïðÿìûå, ìîãóò ïðîèçâîäèòüñÿ â íåñòàíäàðòíûõ âàðèàíòàõ ïî òîëùèíå ñòàëè, òðåáóåìûì ðàçìåðàì âûñîòû è øèðèíû, êà÷åñòâó ìàòåðèàëà, äèçàéíó è õàðàêòåðèñòèêàì ïåðôîðèðîâàííîñòè è òèïó çàùèòíîãî ïîêðûòèÿ. Äîïîëíèòåëüíûå íàöåíêè ïî íåñòàíäàðòíîìó âûïîëíåíèþ, êàê ïðàâèëî, ðàçóìíî ñîîòâåòñòâóþò çàïðîñó.

	Prefabricated sectional metallic cable tray system, in different versions, manufactured according to the IEC 61537
international norm, ideal solution for the distribution, protection and support of the electrical cables in buildings for
civil, tertiary and industrial purposes.
It is easy to pass from one size to another one with the different connection elements which are part of a wide range
of accessories which allow the installation of the system even on winding routes in a rapid way and most of all without
adaptations.
Many elements of the FEMI 3 system, particularly the straight ones, can be produced in extra-standard versions for steel thickness, dimensions B x H, quality of the material, design and characteristics of the perforation and type of surface protection. The additional costs for the extra-standard execution are normally advised on request.