MP Pumps offers various models of both its self priming Flomax Series as well as the end suction S Series with double mechanical seal options. This allows these pumps to perform in applications with intermittent dry run conditions and makes them ideal for handling abrasive fluids.The barrier fluid chamber is filled with high pressure grease providing for inside – out lubrication of the seal faces. These pump types have proven success in various hard – to – handle applications including tank unloading, machine chip conveying, and bentonite handling. 
[bookmark: _GoBack]MP Pumps предлагает различные модели насосов, как самозаливающиеся из серии Flomax, так и одностороннего всасывания из серии S, с возможностью двойного герметизирующего уплотнения. Это позволяет данным насосам функционировать в условиях периодической работы всухую и делает их идеальными для работы с абразивными жидкостями. Камера затворной жидкости наполнена смазочным веществом под высоким давлением для обеспечения внутренней и внешней смазки поверхностей уплотнения. Доказано успешное применение этих насосов в трудных условиях, таких как слив из резервуара, машинное удаление стружки и перекачка бентонита.     

