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ONUC IHOOPMALYIAHWX CUCTEM

Inopmauiiini Tabno

B KOMNEKT NOCTaskn BXOAATS TP  30BMiLIKiX (nepegHiF, GokoBHit Ta 3aaWif) Ta OqUN SHyTpILINI
NPOrpamosaKi UMdposi coiTnoioni expann (LED — expawk), 1O BIAOSPaNAIOTH MAPLIPYT, HOMED
MAPWPYTY | NYHKT NPHIHAUSHKA Ta NPUCTPOEM YNIPABAIHHS, SKIi BCTaHOSMIOETBCA & Kabiki BORA
EKPaKW  SMKOPHCTOSYIOTS OAHOKONOPOSI CBITAOAIOAH BUCOKCH HTEHCBHOCT! 3 LIMPOKUM KYTOM OFAZY
(e menwe 110°). MepeaGaueno asTomaTuHe HaraLTYBaHHA ACKPaBOCTI SIAOGPaENHA iHbOPMALLT, &
SAENHOCT BIA 308HILHIX CBITAOBMX YMOS. Bel CKAIA0SI YaCTUHW, AKI BXOAATS & KOMATEKT Nocrask,
CNPOEKTOBaHI | BMroTOBNEH, AK CTiiki 40 Kpanens | siBPAUT | Tar, W6 BOHM MO  npauposaTH
TIPOTATOM BELOIO exCRAYaTaLiHOTO TepwiNy a8TOByca (10 pokis).

IHBOPMALIA NOAIETHCA YKPAINCBKOIO, BHFATHCSKOKD | IHLIMMMH MOBaMH ( KHPMAMLA | AATHHAUS ), 3 Takok
AOARTKOBUMM CHMBOTaMM, 3aMpOrpaNOBaHMMK  JaOsKKOM. Nepeabauena amiMa  inpopmauii Ta i
TIPOIPAMYBIKKA  JAMOBHMKOM Wa CTaHABPTHOMY OGMagWaWki 13 Ge3KOLTOBWMM  HagaWMAM
BIANOBIANOTO. NPOTPaMHOTO 3aGe3neueHHs.

Mlepuumi - nepeaniii NiTepo-LMGPOBMA expan ( 3670 ) BCTaHOSMOETSCA MA CKIOM Ha nepeaniii
MACTKI 35TOGYC Ha/ SITPOBMHM CHOM i MGE MOXMBICTS NOKa3YBATH MAPLIPYTHY IHGOPMALI0 8 OWH 360
5 453 PAAKE 8 CTaTW4HOMY Pewuni, 360 5 pemmi « Giryuol cTpiuKiny. Mpw SIAOGPaMeHHI indopmaliy Asa
PAAK ~ KOKHMH PAAOK NPOTPAMYETLCA OKPEMO. [a6apHTHI POIMIPH NepeANBOT0 TaBn0 1706 M x 230 s
X50 M. Ta670 mae 16 x 160 LED.

Apyruii — 6oKosi AiTepo-LbpOsMii expan (Tabno ) BCTaOBMOETCA 32 CKOM y Npasilt uacTHi aBTOBYCy
| MG€ MOKIMBICTS NOKa3YBITH MApLIPYTHY IHGOPMALIIO & OAMH 360 B AB3 PAAKA B CTATHAHOMY pemi,
360 5 pewumi « Girysoi crpiunwy. Mpu siaoGpamenni IHGOPMALIT y ABa PAAKS — KOWHMA PAZoK
TIPOTPaMYETSCA OKpEMo. [aBapHTHi po3MipH 6OKOBOT TaGn0 1210 M x 230 Mt x 50 M. Ta6no mae 16 x
96 LED.

‘Therili — 32 expan ( Ta6no ) scTanoBMIOETSCA 33 3aANIM CKOM aBTOBYca | BiAOBpaNGE MAPLIPYTHY
#4OPMaLio (Homep aGo ciMBOn MapLIPYTY). [a6IPUTH POIMIpH  33AHBOTO TaBA0 436 MM X 230 M x 50
M. Tabno mae 16x 32 LED.
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DESCRIPTION OF INFORMATION SYSTEMS

Information boards

The package includes three external (front, side and rear) and one internal programmable digital LED
screens (LED screens), which display the route, route number and destination and a control device that is
installed in the driver's cab. The screens use single-color high-intensity LEDs with a wide viewing angle (at
least 1100). There is an automatic adjustment of the brightness of the information, depending on the
external lighting conditions. All components included in the delivery set are designed and manufactured as
resistant to drops and vibration and so that they can operate throughout the life of the bus (10 years).

The information is provided in Ukrainian, English and other languages (Cyrillic and Latin), as well as
additional characters programmed by the Customer. It is planned to change the information and its
programming by the Customer on standard equipment with free provision of appropriate software.

‘The first - the front alphanumeric screen (board) s installed under the glass on the front of the bus above
the windshield and has the ability to show route information in one or two lines in static mode, or in the
“treadmill” mode. When displaying information in two lines - each line is programmed separately. Overall
dimensions of the front panel 1706 mm x 230 mm x 50 mm. The board has 16 x 160 LEDs.

‘The second - the side alphanumeric screen (board) is installed behind the glass in the right part of the bus
and has the ability to show route information in one or two lines in static mode, or in the "treadmill* mode.
When displaying information in two lines - each line is programmed separately. Overall dimensions of a side
board are 1210 mm x 230 mm x 50 mm. The board has 16 x 96 LEDs.

The third - the rear screen (board) is installed behind the rear window of the bus and displays route
information (number or route symboll. Overall dimensions of the rear panel are 436 mm x 230 mm x 50
mm. The board has 16 x 32 LEDs.




