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A - SAFETY INSTRUCTIONS
1 - Never start the machine before closing the covers of protection
2 - Do not touch the moving parts (chuck, plunger, stone-holder, stone-holder bars, head) while the machine is working.
3 - Before starting the polishing process, make sure that the plunger is correctly fixed onto the chuck.
4 - Never leave the keys on the chuck when the machine is working.
5 - When adjusting the final polishing point, never adjust the sliding bar when the machine is working.
6 - In order to avoid to block the stones on the plunger tip and to break the stones-holder bars, adjust the polishing run at around 7 to 8 mm from the plunger tip.
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B - CONTROL PANEL
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1 -
Adjustment button for pressure of left head

2 -
EMERGENCY STOP button

3 -
Automatic / Manual switch

4 -
For manual position : ON / OFF switch for chuck rotation
5 -
Control button for variation of spindle speeds

6 -
Switch for jack in
7 -
Timer
8 -
Adjustment button for pressure of right head

9 -
Visual display for pressure of right head

10 -
Switch for jack out
11 -
Control button for variation of chuck rotation speeds
12 -
Red light showing end of cycle 
13-
START CYCLE button
14 -
Visual display for pressure of left head
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C - MACHINE OPERATION
C.1 - DESCRIPTION OF THE SYSTEM
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1 -
Sliding bar to adjust final polishing point

2 -
Head
3 -
Screw for adjusting the head
4 -
Clamping gripping jaw (either internal gripping jaw or external gripping jaw)
5 -
Blocking screw for the chuck

6 -
Plunger

7 -
Polishing stones
8 -
Stone-holder bar
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C.2 - SET UP OF THE PLUNGER
1 - Switch the Automatic / Manual button on Automatic and the control button for variation of spindle speeds on the position 1.

2 - Close the safety cover and press the push-button Start cycle.
 3 - When the head is the farthest from the chuck, stop the machine in switching the Automatic /Manual switch on the position Manual.
4 - Choose clamping gripping jaw (either internal gripping jaw or external gripping jaw) and assemble them in the order 1, 2, 3. It is possible to make the chuck rotate manually when the Automatic /Manual switch is on the position Manual by pushing the push button for chuck rotating (the green).
5 - Install the plunger on the chuck and block it.

C.3 - SET UP OF THE POLISHING STONES
We can polish with stones, diamond stones or felts and diamond paste (large assortment specially adapted for the machine available)
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Polishing stones
Felts
Felt-push
Clamping system for the felts
Clamping system for the stones
Felt
Polishing stone
Diamond paste
For the polishing stones, install the clamping system for the stones, install the stones and make them overlenght from the same value.
In order to use felts, disassemble the clamping system for the stones and install the clamping system for the felts with the felt-push. Install the felts, make them overlenght with the same value, place diamond paste on the extremity of the felts and lubricate with a oil-petrol mixture.
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C.4 - ADJUSTMENT OF THE POLISHING ZONE
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Final point of polishing
Stroke
C.4.1 - ADJUSTMENT OF THE FINAL POLISHING POINT
1 - Release the screw so as to adjust the head with an alien key of 6 and move the assembly head-stone-holder bar in the opposite direction from the chuck.
2 - Switch the Automatic /Manual button on Automatic.
3 - Set the control button for variation of spindle speeds on the position 1.

4 - Press the push-button Stat cycle.
5 - When the polishing stones are the nearest from the chuck, stop the machine in switching the Automatic /Manual switch on the position Manual.

6 - Move the assembly head-stone-holder bar until the stones reach the final polishing point and srew the screw in order to adjust the head.
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C.4.2 - ADJUSTMENT OF THE STROKE
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Lubricating taps
Panel control
Handwheel
for stroke
setting
Tank for old oil
1 - Release the knurling button which is in the center of the handwheel for stroke setting.

2 - Switch the Automatic /Manual button on Automatic and set the control button for variation of spindle speeds on the position 1.

3 -* Close the safety cover and press the push-button Start cycle.
4 - When the head is the farthest from the chuck, stop the machine in switching the Automatic /Manual switch on the position Manual.
5 - Adjust the stroke from the polishing stones with the handwheel corresponding with the head with the plunger.

BE VERY CAREFUL NOT TO HAVE A TOO LONG STROKE. IN THIS CASE, THE STONES SHOULD BE BROKEN BY THE EXTREMITY OF THE PLUNGER AND THE STONE HOLDER BAR. SHOULD BE FOLD UP.
ALWAYS FORESEE SOME MILLIMETERS SECURITY AT THE EXTREMITY OF THE PLUNGER.
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- When the stroke is well adjust, srew the knurling button which is in the center of
the handwheel for stroke setting.
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C.4.3 - ADJUSTMENT OF THE TIMER
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Timer stop
Timer in working
Clamping ring
Setting time
coefficient
(x0.l ou xl)
Setting
Hour,
Minute or
Second
Hour,
Minute or
Second
display
Time
coefficient
display
So as to set the timer, lift up the clamping ring, choose the time unit you want (we have the choice between hours, minutes or seconds), and the time coefficient (either 1, or 0.1). In order to change these values, use a small srew-driver and make rotate the setting knurling.
Choose the value you want by turning the dial until the pointer is on the good number. When all the settings are good, install the clamping ring.
The green light will bright when the timer will operate.
The red ligth will bright only when the timer will arrive on zero.
9
C.4.4 - POLISHING
After setting, install correctly the lubricate pipe, close the safety cover. After:
1 - Switch the Automatic /Manual button on Automatic.
2 - Set the polishing time on the timer.
3 - Press the push-button Start Cycle.
4 - Press the push-button Switch for jack in
5 - Set the spindle and the chuck rotation speeds.

6 - Open the oil tap and let the oil dripfeed.

7 - Adjust the polishing pressure by drawing the adjustment button (number 1 & 8 on the scheme) up to the top until the value of the required pressure, indicated on the manometer, is reached. Then push the adjustment button down to the bottom.
To stop the machine, press the push-button Switch for jack out and switch the Automatic /Manual button on Manual
Please note: if we don't stop the machine voluntarily, it will stop when the timer will be on 0. At this time, the red signal end of cycle will light and lubrication will stop automatically.
D - MAINTENANCE
- Check the level of oil lubrication.
- Lubricate the bearings feating, once a month.
- Check the level of oil in the compressor (a bottle is supplied with the machine).
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