Complete linear filling machine is used to fill containers with liquid and viscous products such as household chemistry, agrochemistry, auto chemistry, oils and essential oils.
 
Characteristic features of complete linear filling machine:
·         actuating units are arranged linearly along the conveyor;
·         adjustable railings;
·         incrementally the corresponding process stages take place: filling, capping, labeling.
 
Filling may be realized by means of the following types of filling machines: piston filling machine, overflow filling machine, servo pump filling machine, net-weigh filling machine, time gravity filling machine.
As a result of customized selection of filling method according to the customer preferences, specifity of the production, product features and containers form factor, filling range 0,5…30 l with accuracy up to 0,5…1,5% may be achieved.
 
Operating peculiarities of filling line:
·         bottles (cans) are put on the conveyor;
·         move automatically to the filling site;
·         bottles (cans) presence at the filling site is determined by means of variable photosensors;
·         bottles are filled automatically by means of filling machine;
·         filled bottles (cans) move further to capping, labeling and other processing steps.
 
Depending on the customer’s preferences and his planned budget bottles may be fed to the conveyor:
·         manually by the operator;
·         by means of incoming turntable;
·         by means of automatic bottle management.
 
Advantages:
·         regulated filling range 0,5...30 l;
·          type of cap;
·         labels quantity;
·         proficiency of attending personnel.
 
 
Contact us, and we’ll do our best to successfully deal with your task!

