	Трубопроводный транспорт был и остается достаточно серьезной проблемой для компаний, занятых    транспортом углеводородного сырья.  
При трубопроводном транспорте нефти возникают серьезные проблемы из-за кристаллизации парафинов и возрастания вязкости нефти: повышаются давление в трубопроводе, расход электроэнергии на оборудование прокачки и их износ, уменьшается пропускная способность трубопровода. В холодных климатических условиях транспорт нефти еще более осложняется из-за парафиноотложений непосредственно на внутренних стенках трубопроводов, то есть сужается поперечное сечение нефтепровода и как следствие снижается производительность. 
Из многочисленных способов борьбы с парафинистыми отложения при транспортировке нефти наиболее эффективным признано введение химических реагентов, предотвращающих или ингибирующих отложение парафинов. В качестве таких реагентов используют поверхностно-активные вещества и депрессорные присадки (ДП). Преимущество присадок заключается в том, что, помимо предотвращения отложений парафинов, они улучшают свойства нефти, снижают температуру потери текучести, что важно при дальнейшем ее транспортировании. Одним из способов улучшения   свойств высоковязких и высокозастывающих нефтей являетсяввод в состав их синтетических компонентов, в качестве которых могут быть использованы низкомолекулярные олефины, длиноцепные альфа-олефины и их соолигомеры.  При этом носителями депрессорных свойств выступают длинноцепные алкильные радикалы, ароматические углеводороды с длинными алкильными радикалами и гетероциклические соединения.  

	Pipeline transportation remains a serious problem for companies engaged in the transportation of hydrocarbons.  
In the pipeline oil transportation, serious challenges occur due to the crystallization of paraffin and the increase in the oil viscosity: the pressure in the pipeline increases, as well as the power consumption for pumping equipment and its deterioration, the throughput of the pipeline decreases. Oil transportation is even more challenged during cold weather due to paraffin deposition directly on the inner walls of pipelines, that causes the narrowing of cross-sectional area of the oil pipeline, and, as a result, reduces efficiency. 
[bookmark: _GoBack]The addition of chemical reagents that prevent or inhibit the deposition of paraffin is considered as the most effective among many methods to deal with paraffin deposits during oil transportation. Surfactants and pour point depressants (PPD) are used for this purpose. The advantage of PPD is that they not only prevent the paraffin deposition, but also improve the properties of oil, reduce the pour point, which is important for further oil transportation. One of the methods to improve the properties of high-viscosity and high pour point oils is the addition of synthetic components into their composition, which can be used as low-molecular olefins, long-chain alpha olefins and their co-oligomers.  Long-chain alkyl radicals, aromatic hydrocarbons with long alkyl radicals and heterocyclic compounds act as carriers of depressant properties.



