1. Перекласти на українську

In compliance with CE 428/2009 norm which establishes the community exports control over dueal use products and technologies, we hereby declare that the herein listed products of this document are constitued by equipments for the dosing and control of liquids and their relative accessories and spare parts and therefore destinated to exclusiv civil use.

2. Перекласти на англійську
Дистриб’ютор буде докладати всіх зусиль, щоб активно поширювати і продавати Товари на призначеній йому Території і Ринкових секторах; набрати відповідний штат спеціалістів з продажу, розвинути дилерську мережу та знайти оптовиків; задовольняти всі запити на Товари від потенційних покупців на призначеній території; інформувати Виробника про ринкові умови, можливості, попит на продукцію і проблеми ринку; інформувати  Виробника про дилерів і оптовиків на його території; ознайомлювати покупців з принципом роботи обладнання та поводження з ним, надавати технічну підтримку для всіх клієнтів; відповідати та дотримуватися  політики продажів Виробника; і вести свій бізнес таким чином, щоб в повній мірі розвивати і захищати імідж і торгову марку Виробника на призначеній території.

3. Перекласти на українську

4. The pump is provided with a connector for connection to an external water meter which can provide a series of contacts proportional to the amount of liquid that must be threated. For each contact,  received from the meter, the pump delivers a number of injections directly proportional to the set value in “ml” (millilitres) requested by the user. They display shows in a dynamic manner the amount dosed in “ml”.

5. Перекласти на англійську
Сильфонные торцовые уплотнения валов  – это компактное торцевое уплотнение модульного типа с одной центральной пружиной и эластомерным сильфоном, которое обеспечит максимальную эффективность и работу вашего оборудования в любых условиях.

Торцевые уплотнения с цилиндрической пружиной. Уплотнение с уплотнительным кольцом круглого сечения.
Этот тип механических уплотнений идеально подходит для широкого применения в различных режимах работы торцевых уплотнений, начиная от водоснабжения и до применения в нефтехимической промышленности или других  приложениях, требующих высокую надежность и качество насосного оборудования.

1. Перекладено на українську
Згідно з нормою CE 428/2009, яка встановлює суспільний експортний контроль над товарами та технологіями подвійного призначення, цим документом ми оголошуемо, що перераховані у цьому документі товари призначаються обладнанням для обліку та контролю рідин та відносних до них аксесуарів і запасних частин і, отже, призначаються виключно для цивільного використання.

2.  Перекладено на англійську

Distributor shall exert every effort to active dissemination and selling Goods on the designated Territory and Market sector; to recruit relevant staff of sale specialists, to develop dealer network and find wholesalers; to satisfy all the requests for Goods from potential buyers on the designated territory; to inform Manufacturer about market conditions, opportunities, demand for products and market issues; to inform Manufacturer about dealers and wholesalers on his territory; to acquaint buyers with operation principle of equipments and handing with it, to provide technical support for all customers; to align and adhere to Manufacturer sales policy; to conduct business to fully develop and  protect the image and trademark of Manufacturer  on the designated territory.  
3. Перекладено на українську

Насос подається з роз’ємом для підключення до зовнішнього водоміру, який може забезпечити низку контактів, пропорційну кількості рідини, яка має бути пропущена. Для кожного контакту, отриманого від вимірювача, насос забезпечує ряд вливань прямо пропорційних до встановленного в “мл” (мілілітри) значення, вказаних користувачем у запиті. Дисплей динамічним чином відображає кількість дозованої рідини в “мл”.  
4. Перекладено на англійську
Bellows face seal are a compact modular type face seal with a central spring and elastomeric bellows, which shall provide the highest efficiency and equipment performance in any setting. 

Face seals with a cylindrical spring. Seal with a sealing O-ring.
This type of mechanic seals is impeccable for widespread use in various operation modes of face seals, ranging from water supply to use in oil industry or other attachments, what require high reliability and quality of pumping equipment.
