	DEEPLOW - Платформа мониторинга и контроля заглубления орудия

Deeplow Уникальная технология для измерения глубины погружения сельскохозяйственного орудия в почву

Уникальная технология Deeplow позволяет с высокой точностью контролировать глубину погружения орудий при обработке почвы. Набор сенсоров подбирается с учетом конструктивных особенностей агрегатов.

 Deeplow решение измеряет глубину погружения орудий посекционно и учитывает индивидуальные особенности именно вашей техники. Все данные от сенсоров поступают в центральный контроллер – настоящий мозг системы. 


Большим преимуществом решения Deeplow является обработка и фильтрация полученных данных прямо на борту агрегата. Таким образом, достигается высокая точность измерений даже при попадании растительных остатков в область измерения.
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Глубина погружения сельскохозяйственного орудия в почву

Контроль глубины обработки, заданной регулировками агрегата

 Наличие контроллера позволяет производить дополнительную математическую обработку измерений на борту

Определение подъёма и опускания агрегата на разворотах и при транспортировке

Решение подходит для различных орудий и конфигураций агрегатов


	DEEPLOW - Tool Penetration Monitoring and Control Platform

Deeplow  - Unique technology for measuring the depth of penetration of agricultural implements into the soil

The unique Deeplow technology allows you to control the depth of implements immersion during tillage with high accuracy. A set of sensors is selected taking into account the design features of the units.


The Deeplow solution measures the penetration depth of the implements by sections and takes into account the individual characteristics of your equipment. All data from the sensors are sent to the central controller - the real brain of the system.


The big advantage of the Deeplow solution is the processing and filtering of the received data directly on the unit board. In this way, high measurement accuracy is achieved even if plant residues enter the measurement area.




Implement depth control sensors
Controller
The depth of agricultural implements immersion into the soil

Control of the depth of processing, set by the adjustments of the unit

The presence of a controller allows for additional mathematical processing of measurements on board


Determination of the lifting and lowering of the implement during headlands and during transport

Solution is suitable for various implements and implement configurations



	INSMARTRAIN - Платформа мониторинга и удаленного управления дождевальными машинами
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InSmartRain Аппаратное решение подходит для круговых и фронтальных дождевальных машин любых марок

Платформа InSmartRain: 
• удаленное управление (запуск, остановка, норма выливания, разрешение включения пушки, включение подачи удобрений, включение подачи воды); 
• расчет показателей работы по секторам полива; 
• расчет показателей потребления воды по паспортным характеристикам или расходомеру;
расчет показателей полива в мм дождя;
 
• сигнализация об аварии;
 • фиксация периодов работы водяной пушки (при наличии); 
• фиксация движения без воды в магистрали; 
• гибкие настройки под любую конфигурацию дождевальных машин.


InSmartRain сенсорная панель и контроллер устанавливается вместо стандартной панели управления Reinke и подключается в стандартный разъем. Гарантия производителя сохраняется.
	INSMATRAIN - Platform for monitoring and remote control of center-pivot irrigation systems’
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[bookmark: _GoBack]InSmartRain is a Hardware solution suitable for all brands of linear and central pivot irrigation systems’

InSmartRain Platform:
• remote control (start, stop, pouring rate, permission to turn on the end water gun, turn on the fertilizer supply, turn on the water supply);

• calculation of performance indicators for irrigation sectors;
• calculation of water consumption indicators according to passport characteristics or flow meter;
calculation of irrigation indicators in mm of rain;
• alarm about the accident;
  • fixing the periods of operation of the end water gun (if available);
• fixation of movement without water in the highway;
• flexible settings for any configuration of center-pivot irrigation systems’.

The InSmartRain Touch Panel and Controller installs instead of the standard Reinke control panel and plugs into a standard connector. The manufacturer's warranty remains.



	INSMARTAGRO - Платформа мониторинга влажности и температуры почвы
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InSmartAgro LoRaWAN передача данных от точки измерения. Измерение влажности и температуры на двух глубинах.

Платформа InSmartAgro: 
• мониторинг влажности почвы на разных глубинах 
• мониторинг температуры почвы на разных глубинах 
• гарантированная автономная работа без замены батарей в течение 1 года
 • LoRaWAN передача данных мониторинга почвы и без GSM канала 
• интеграция с Wialon - IoT платформой для отображения показаний 
• мобильное приложение для просмотра данных с датчиков прямо на поле (чтение через NFC или штрих-код) фиксации координат точки при инсталляции
 • хранение данных за всю историю наблюдений 
• интеграция с платформой Cropio в первом квартале 2022 года

InSmartAgro станция измерений поддерживает работу с лучшими датчиками влажности почвы ведущих производителей.
	INSMARTAGRO - Soil Moisture and Temperature Monitoring Platform



Selecting an installation site by GPS
Selecting the measurement period
Reading data remotely and via NFC tag smartphone

InSmartAgro LoRaWAN data transfer from the measurement point. Measurement of humidity and temperature at two depths.

InSmartAgro platform:
• soil moisture monitoring at different depths

• soil temperature monitoring at different depths
• Guaranteed autonomy without battery replacement for 1 year
 • LoRaWAN transmission of soil monitoring data without a GSM channel
• integration with Wialon - IoT platform for displaying readings
• a mobile app for viewing data from sensors directly on the field (reading via NFC or a barcode) fixing the coordinates of a point during installation
 • storage of data for the entire history of observations 
• integration with the Cropio platform in the first quarter of 2022

InSmartAgro measurement station supports the best soil moisture sensors from leading manufacturers.



