

    A port is one of the main elements of transport hubs which joins sea lanes with inland communications. Historically ports have always been hives of activity. News and tales from faraway lands were told here, one could find a job or have a chat here. Every merchant made it a rule to send its agents to ports and very often important trade contracts were concluded there.
    
The role of ports is not limited by the functions of the most important element of the transport system. They influence not only the economics of a certain region, but also the national economic in general.
   
 This is still up-to-date. So nowadays a port is a big transport enterprise, a complex of engineering structures and equipment for fast and efficient offload, passenger shipping, safe turn around, ground vessel services and repair. 
    
Proper arrangement of the port is one of the focal tasks which should be solved on the stage of its designing. The port may be located in rather favourable geographic conditions, but absence of a proper link between certain components can affect their interaction and efficiency of operating the port in general. Ergonomics of cargo turn-over, environmental safety and occupational health so as cost efficiency should be taken into consideration. Improper arrangement and location of its components can affect the environment at the seaside nearby the port. 
   
 Port installations include passenger ship terminals, shiprepairing shops, warehouses, moorings, ferry crossings etc. During arrangement zonation and regionalization of the so-called High-Security Area should be considered. It consists of the operational zone, industrial zone and general port zone.
The operational zone consists of technical objects and facilities for reloading. Proper arrangement is very important here. Also the types of cargo should be considered.
Warehouses, trackways and industrial auxiliary objects are located in the industrial zone.
The general port zone consists of objects and services for general port activity and ground vessel services. All these zones are usually walled in.
[bookmark: _GoBack]Judging from the conditions of rational arrangement of the port area, cargo terminals of similar specialization should be located in one place by combining them into individual specialized zones such as zones for general cargos, bulk dry cargos, timber cargos, grain cargos, bulk liquids, containers and other cargos.
So we’ve considered the main port installations and objects so as the nuances of their proper arrangement. Hope this video was useful for you! Subscribe to our channel and like this video!
