Эксплуатация и обслуживание системы обращения с ТП

ТО.Т2.ПЦ2 Описать порядок приемки ТП в ХОЯТ-2 
В связи с тем, что окончательно не решен вопрос с поставщиком пустых топливных патронов,
предполагается, что пустые топливные патроны с крышками доставляются в ХОЯТ-2 в металлических контейнерах емкостью по 45 штук, установленными на железнодорожной
платформе. Габаритные размеры контейнера примерно 3900х1200х600 мм.
Вес контейнера с пустыми патронами около 1000 – 1200 кг. Перегрузка контейнеров с железнодорожной платформы на грузовой автомобиль осуществляется на участке перегрузки на
территории ХОЯТ-2 с помощью вилочного погрузчика. Затем контейнеры грузовым автомобилем
транспортируется в склад пустых патронов. В складе контейнеры штабелируются. По высоте контейнеры устанавливаются не более 4 штук. Ожидается, что в складе будет находиться годовой
запас пустых патронов (5000 штук), что составляет около 100 контейнеров.
По мере использования пустых топливных патронов пустые контейнеры отправляются на
утилизацию, как нерадиоактивные отходы.

ПЕРЕВОД
OPERATION AND MAINTENANCE OF FT HANDLING SYSTEM

[bookmark: _GoBack]Describe the sequence of FT receipt in ISF-2 25 min.
Considering that the question with deliverer of empty fuel tubes isn’t finally resolved, is expected that empty lidded fuel tubes are delivered to ISF-2 in metal canisters with a capacity of 45 pieces, set at railway platform. Dimensional specifications of canister are about 3900x1200x600 mm. The canister’s weight with the empty tubes is for about 1000-1200 kg. Canister transfer from the railway platform to the auto truck is carried out on the site of transfer in the territory of ISF-2 with a forklift. Then canisters transport with auto truck to the ware house of empty tubes. In a ware house canisters are stacked. On hightwise canisters are setting up not over 4 pieces. It is expected that in a warehouse will be the year’s supply of empty tubes Shows and comments slides №24-27 « Sequence of FT receipt in ISF-2»  (5000 pieces), which amounts about 100 canisters. While using of empty fuel tubes empty canisters are sent for utilization as non-radioactive waste.


