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Always unplug and let cool before cleaning.

FOR A LIGHT CLEANING:

18. Using dishcloth or sponge with a mild dishwashing detergent and warm water, wipe

glass bowl, lid and fan housing clean.

19. Rinse glass bowl well to remove all detergent.

NOTE:
- Never immerse the lid in any liquid.
If scrubbing is necessary, use a nylon or polyester mesh pad.
- Do not use a steel wool pad or abrasive material.
- Never use solvents or cleaning powers.

- Be careful no to get any liquids inside the lid.
TO SELF-CLEAN GLASS BOWL:

1. Add 4cm(1 1/2”) of water and mild detergent.

2. Replace the lid.

3. Set thermostat at “wash” and set timer for 10 minutes.
The hot air circulation creates a turbo wash action that removes even baked on
residues. The wire rack and other dirty parts may be left in convection roaster for
pre-washing during this process.

4. When the timer switches “off”, remove the lid and rinse bowl in warm water to
remove all soap residue. If the convection roaster is particularly dirty, replace to and

switch on for another 2 or 3 minutes.

NOTE: Do not fill with liquid above the water line marked on the bowl.

RECIPES

Please refer to the Quick Reference Card for general guidelines regarding cooking time
and methods.
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Before cooking with your Convection Roaster for the first time:

Wipe glass bowl clean with a damp sponge
Place lid centrally and securely onto bowl
Plug the cord into power point

Set thermostat to 250°C

Set timer for 5 minutes to remove any lubricants from the element (you will notice a
slight burning odor)

Allow to cool for 5 minutes with top unit remove.

NOTE: Be careful to put the sides at least 3" from any other surface

1.

Place Food Centrally in the bowl on the dual height rack keeping the food

approximately 1 to 1 1/4” from the glass wall to allow maximum air circulation.
Place lid on bow.

3. Insert the plug firmly into the wall outlet.

NOTE: Tpe thermostat
element ™

The timer Will switch “off*
momentarily to alert you th,

Set the thermostat and timer as required. Check recipe or the quick reference card for
recommended cooking temperature and time.

Your convection Roaster will quickly heat up to the set temperature and maintain this

temperature until the selected time expires. The fan and element will then both switch
“off”

accurately controls the temperature by switching the
off", you will notice the temperature pilot light blinking “on” and “off”

ill sound
after the present time period has passed and a bell Wil S
at the cooking time is over.
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OPERATING lNSTRUCTlONS
Before cooking with your Convection Roaster for the first time:

. Wipe glass bowl clean with a damp sponge

. Place lid centrally and securely onto bowl

- Plug the cord into power point

. Set thermostat to 250°C

- Set timer for S minutes to remove any lubricants from the element (you will notice a
slight burning odor)

- Allow to cool for 5 minutes with top unit remove.
NOTE: Be careful to put the sides at least 3’ from any other surface

Place Food Centrally in the bowl on the dual height rack keeping the food

approximately 1 to 1 1/4” from the glass wall to allow maximum air circulation.
2. Place lid on bowl.

Insert the plug firmly into the wall outlet.

Set the thermostat and timer as required. Check recipe or the quick reference card for
recommended cooking temperature and time.
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Ронсон

Інструкції щодо операцій

Ронсон

Інструкції щодо операцій

Перед готуванням з вашим паровим грилем вперше треба знати: 

· Витріть скляну чашу вологою ганчіркою

· Встановіть кришку по центру та пляму на чашу

· Вставте вилку в розетку

· Наставте важіль температури на 250 градусів

· Наставити таймер на 5 хвилин щоб усунути будь-які лубриканти з пристрою (ви помітите легкий аромат горящого)

· Дайте охолодитися 5 хвилин повністю

Примітка: Будьте обачними щоб розмістити сторони по крайній мірі на три сантиметри один від одного від інших поверхонь.

1. Розмістіть їжу по центру чаші на подвійній решітці зберігаючи їжу на відстані ні один 14мм від скла щоб дозволити максимальну циркуляцію повітря. 

2. Розмістить кришку на чаші

3. Обережно вставте вилку в розетку

4. Наставте термостат на таймер як треба. Перевірте рецепт чи картку рецептів щоб готувати ти з потрібною рекомендованою температурою та часом. 

5. Ваш аерогриль швидко нагрівається до заданої температури і підтримуватиме цю температуру протягом заданого часу.

Машина та тени вимкнувся тоді разом. 

Примітка: термостат власне контролює температуру коли виключає пристрій ви помітите як індикатор температур блимає увімкнено та вимкнено. Таймер вимкнеться після того як  якийсь відрізок часу пройде та звучить дзвіночок , звучить щоб повідомити що час готування вийшов.

Експлуатація

Завжди від'єднайте від електропостачання та дайте охолонути перед тим як мити.

 Для легкої очистки:

Використовуючи ганчірку чи губку та помірний дезінфекційний засіб й  теплу воду витріть скляну тару, кришку та нагріваючий елемент (сухим).

Примітка:

· Ніколи не занурюйте кришку жодну з рідин. Якщо потрібно її очищення використовуйте нейлонову ганчірку чи поліестер. 

· Не використовуйте скребок (сталевий) чи агресивний матеріал.

· Ніколи не використовуйте розчинників.

· Будьте обачні аби не допустити попадання жодної рідини всередину кришки. 

Самоомиваюча чаша:

1. Додайте води на рівень 4 см в чашу та  миючого засобу

2. Встановіть кришку

3. Задайте на термостаті функцію "миття" на час 10 хвилин. 

Циркуляція гарячого повітря створює турбомиття та забирає забруднення та накип.

Своєрідна сітка зі сміття чи інші брудні частинки можуть залишатись в  жаровні під час цього процесу. 

4. Коли таймер вимикається покрутить кришку та занурте чашу в теплу воду щоб забрати всі мильні елементи. Якщо жаровня частково засмічена встановіть її знову на миття ще якісь дві три хвилини. 

Примітка: Не вживайте більше води ніж є позначка на часі!!

