The Analytic Splitter (AS-xx) splits off a certain fixed percentage (xx) for the radioactivity measurement. This partial eluate flow is mixed with liquid scintillator by the T-mixer and passed on to the admixture cell of the HPLC Monitor. The other share of the eluate is passed on to the fraction collector. 
Standard versions of the AS-xx have a splitting ratio of 15%, 25%, 33% and 50%. These percentages define the share of the eluate which is passed on to the radioactivity cell.
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Аналитический Разделитель (АР-XX) отделяет определенный фиксированный процент (xx) для измерения радиоактивности. Эта  частичная подача  элюата смешана  с жидким  сцинтиллятором T-микшером и переходит  дальше в ячейку  примеси монитора ВЭЖХ. Другая часть  элюата выдерживается  в ячейке фпакций. 
Стандартные версии АР-хх имеют коэффициент  15%, 25%, 33% и 50%. Эта процентная концентрация определяет долю элюата, которая переходит  в радиоактивную ячейку.
