Оригинал
Ventilation systems EASYAIR are the economy and efficiency
Founded by Alois Kober in distant 1931, small company passed the way from metalworking workshop to one of the leading german machine-building concerns AL-KO Kober during the years of its existence. Purchasing in 1975 the company GmbH "polar-Lufterhitzer-Werkes" (now AL-KO THERM GmbH) concern (trust) entered the world market of ventilation equipment.
Ventilation installations, produced by concern nowadays, are developed as one of the elements of energy-saving technologies, after all the lack of energy carriers is one of the stumbling blocks in the modern world.
Let’s consider the ventilation systems in detail. In general case, ventilation is divided on exhaust ventilation, input (forced, supply) ventilation and combined extract and input ventilation. The exhaust ventilation – the air is deleted from areas by force, and the fresh air enters as gravity flow by created vacuum. In input scheme the air from outside is injected in the area, and the old one is displaced from it by the difference in pressures through the air holes. In both cases the warm air is displaced by the cool one that needs heating. In essence, the heat is used on street’s heating that result in great consumption of energy carrier. Combined extract and input ventilations with heat recovery are devoid of this defect, and exactly such systems concern AL- KO Kober produces, more exactly, its subdivision – a company ALKO THERM GmbH.
Recovery – is the process of heat utilization of displaced air and the use of this heat on heating the fresh air, injected in the area. The main device, on which efficiency of this process depends, is the heat exchanger. In units of EASYAIR, proposed by concern AL-KO Kober, the heat exchangers of the rotor and apron types are used.
The use of these systems allows to cut down the expenses on heating 5-6 times. The types of heat exchangers of EASYAIR have their own advantages and defects, which we shall consider below.
The highest efficiency possess the heat exchangers of rotor type, in addition they are the most compact. For comparison – unit RO-01 with rotor type of heat exchanger has efficiency 90% and the length 1.5 meters, when corresponding by type RL-01 with apron type of heat exchanger has efficiency near 85% and size in length – more than 2 meters. Rotor type of heat exchangers do not have problems with condensate separation and accordingly, are not subjected to icing, which is one of the serious problems while using apron type of heat exchangers. Ability of units of EASYAIR with rotor type of heat exchanger to bear rather serious frosts without additional energy losses on heating the plates do them more needed in terrains with cool climate. Main defect – impossibility of full division of the flows of displaced and entered air, that’s critical for the situation with unpleasant scent and bad admixtures removing from the room. In addition heat exchangers of the rotor type are more noisy – an average level of noise of the same RO-01 is around 80 Db against 75 Db of RL-01 with heat exchanger of apron type. Efficiency of recuperators of RO-serie is from 650    (RO-01) to 13 thousands of cubic meters per hour (RO-09).
As advantages of heat exchangers of apron type are, first of all, relatively unpretentiousness in service and usage, lower system cost. As it is noticed above, units of EASYAIR with heat exchangers of apron type of RL-serie provide full division of the airstreams that makes them more suitable for systems of ventilation in cafe and restaurants, some productions, rooms of sanitary-hygienic purpose. The greatest defect is the condensate, that conglomerates on heat exchanger plates and results in icing while strong chill. To prevent this, units of RL-serie foresees the variant of package with additional radiator with inspection sensor of freezing.
The ventilation systems EASYAIR with recuperation are equipped with reliable and simple in use automatics, providing the remote control. Different variants of both series recuperators’ package – RO and RL – can provide the additional heating devices for use of the system of ventilation as convective heating, additional inspection parameter sensors of the system itself and environment, gate valves.
The line of the ventilation systems EASYAIR of RO and RL-series with possibility of packaging with additional devices and functions allows to choose the most optimum variant of ventilation practically for any room, and about quality and reliability of technology from Germany does not need to speak – it’s all recognized fact.

Перевод

Вентиляционные системы EASY AIR® - экономия и эффективность
Основанная АлоисомКобером в далеком 1931 году небольшая фирма за годы своего существования прошла путь от слесарной мастерской до одного из ведущих немецких машиностроительных концернов AL-КО Kober. С приобретением в 1975 году компании GmbH "polar-Lufterhitzer-Werkes"(нынеAL-КО THERM GmbH) концерн вышел на мировой рынок вентиляционного оборудования.
Вентиляционные установки, выпускаемые концерном в настоящее время, разрабатываются как один из элементов энергосберегающих технологий, ведь нехватка энергоносителей – один из камней преткновения в современном мире.
Рассмотрим вентиляционные системы подробнее. В общем случае, вентиляция делится на вытяжную, приточную и приточно-вытяжную. Вытяжная – воздух принудительно удаляется из помещений, а свежий поступает самотеком за счет создаваемого разрежения. При приточной схеме воздух извне нагнетается в помещение, а старый вытесняется из него за счет разницы давлений через отдушины. В обоих случаях теплый воздух замещается холодным, нуждающимся в подогреве. По сути, тепло расходуется на отопление улицы, что приводит к большому расходу энергоносителя. Этого недостатка лишены приточно-вытяжные системы с рекуперацией тепла, и именно такие системы и производит концерн AL-КО Kober, точнее, его подразделение – фирма ALKO THERM GmbH.
Рекуперация – это процесс утилизации тепла удаляемого воздуха и использование этого тепла на обогрев свежего воздуха, нагнетаемого в помещение. Главным устройством, от которого зависит эффективность этого процесса, является теплообменник. В агрегатах EASYAIR®, предлагаемых концерном AL-КО Kober, используются теплообменники роторного и пластинчатого типов.
Использование этих систем позволяет сократить расходы на отопление в 5-6 раз. Типы теплообменников EASYAIR® имеют свои достоинства и недостатки, которые мы рассмотрим ниже.
Самым высоким КПД обладают теплообменники роторного типа, к тому же они наиболее компактны. Для сравнения – агрегат RO-01 с роторным теплообменником имеет КПД в 90% и длину 1.5 метра, тогда как у соответствующего по классу RL-01 с пластинчатым типом теплообменника – КПД порядка 85% и размер в длину – более 2 метров. У роторных теплообменников – нет проблем с выделением конденсата и соответственно, они не подвержены обледенению, которое является одной из серьезных проблем при использовании теплообменника пластинчатого типа. Способность агрегатов EASYAIR® с роторным типом теплообменника выдерживать довольно серьезные морозы без дополнительных энергозатрат на прогрев пластин, делают их весьма востребованными в местностях с холодным климатом. Главный же недостаток – невозможность полного разделения потоков удаляемого и приточного воздуха, что критично для ситуации с удалением неприятных запахов и вредных примесей из помещения. К тому же роторные теплообменники более шумные – средний уровень шума того же RO-01 составляет порядка 80 Дб относительно 75 Дб у RL-01 с пластинчатым теплообменником. Производительность рекуператоров серии RO составляет от 650 (RO-01) до 13 тыс. кубометров в час (RO-09).
К достоинствам пластинчатых теплообменников стоит отнести, прежде всего, относительную неприхотливость в обслуживании и эксплуатации, более низкую стоимость системы. Как замечено выше, агрегаты EASYAIR® с пластинчатыми теплообменниками серии RL обеспечивают полное разделение воздушных потоков, что делает их весьма удобными для систем вентиляции кафе и ресторанов, некоторых производств, помещений санитарно-гигиенического назначения. Самый большой недостаток – конденсат, скапливающийся на пластинах теплообменника и приводящий к обледенению в сильные холода. Чтобы предотвратить это, агрегаты серии RL предусматривают вариант комплектации дополнительным калорифером с датчиком контроля замерзания.
Вентиляционные системы EASYAIR® с рекуперацией оснащены надежной и простой в использовании автоматикой, предусматривающей дистанционное управление. Различные варианты комплектации рекуператоров обеих серий – RO  и RL – могут обеспечить дополнительные нагревательные устройства для использования системы вентиляции в качестве конвективного отопления, дополнительные датчики контроля параметров самой системы и окружающей среды, запорные клапаны.
Ряд вентиляционных систем EASYAIR® серий RO и RL с возможностью комплектации дополнительными устройствами и функциями позволяет выбрать наиболее оптимальный вариант вентиляции практически для любого помещения, а уж о качестве и надежности техники из Германии не стоит и говорить – это всеми признанный факт.



