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TYPE PROCEDURES OF REPAIRING DOORS, BLISTERS, EMERGENCY EXIT HATCHES, SKIN AND MAIN FRAME OF FUSELAGE

1. General

This section comprises typical methods of repairing doors, sliding blisters and emergency exit hatches.
The layout of sliding blisters, sliding doors and emergency exit hatches in the article is shown in Fig. 1201.
The list of typical procedures of repairing doors, blisters and emergency exit hatches is given in Table 1202.

	Table 1202
	- List of typical procedures of repairing doors, sliding blisters, emergency exit hatches, skin and main frame of fuselage



	Description
	TС No.
	Pages
	Remarks

	Typical repair of  skin, doors, blisters and emergency exit hatches
	1201
	1201 to 1216
	Figs 1202, 1203, 1204, 1205

	Typical repair of  elements of inner set of doors, blisters and emergency exit hatches
	1202
	1217 to 1219
	Fig. 1206

	Typical replacement of cables, blister, doors and lock of emergency exit hatch window
	1203
	1220 to 1224
	

	Typical repair of load-bearing fuselage main frame
	1204
	1225 to 1234
	Figs 1207 thru 1211

	Typical repair of external skin and load-bearing package of weld-bonding of main frame
	1205
	1235 to 1236
	

	Typical repair of webs of frames and longitudinal beams in places of breaches with dia. from 20 to 40 mm
	1206
	1237 to 1239
	

	Typical replacement of reinforcing plate, fitted during previous repair due to emerging crack
	1207
	1240 to 1241
	Fig. 1212

	Typical replacement of skin portion between neighbor frames and stringers 
	1208
	1242  to 1243
	

	Typical repair of fuselage external skin in case of lack of access for riveting.  Arrangement of temporary hatch
	1209
	1244 to 1247
	Fig. 1213

	Typical repair of sealing elements
	1210
	1248 to 1250
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	Fig. 1201 Layout of Blisters, Doors and Emergency Exit Hatches







Table 1202 –Parts List to Figure 1 –Layout of blisters, doors and emergency exit hatches

	Item No.
	Description of assembly, unit, part
	Drawing No.
	Qty per accessory
	Remarks

	1
	Fuselage middle section
	8АМТ-0300-00
	1
	(Ref. Section 053.10.20)

	2
	LH sliding door
	8АТ-0338-00
	1
	(Ref. Section 052.10.10)

	3
	Sliding blister 
(LH/RH)
	8АТ-0200-400-1/-2
	2
	(Ref. Section 052.20.00)

	4
	RH sliding door
	8АТ-0338-1000.973
	1
	(Ref. Section 052.10.40)

	5
	Emergency exit hatch window
(big or small)
	8АМТ-0300-800 (small)
8АМТ.0385.2000 (big)
	3

3
	(Ref. Section 052.20.30)

	6
	Emergency exit hatch
	8АМТ.0700.100
	1
	(Ref. Section
052.30.11)

	7
	Cargo door panels

	8АТ.0700.00
	1 LH
1 RH
	(Ref. Section 052.30.10)
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ТИПОВІ ПРОЦЕДУРИ З РЕМОНТУ ДВЕРЕЙ, БЛІСТЕРІВ, АВАРІЙНИХ ЛЮКІВ, ОБШИВКИ І КАРКАСУ ФЮЗЕЛЯЖУ

1. Загальні положення

Ця секція включає в себе типові методи ремонту дверей, зсувних блістерів та аварійних люків.
Схема зсувних блістерів, зсувних дверей та аварійних люків показана в цьому пункті на Мал. 1201.
Список типових процедур ремонту дверей, блістерів та аварійних люків наданий в Таблиці 1202.

	Таблиця 1202
	- Список типових процедур ремонту дверей, зсувних блістерів, аварійних люків, обшивки та каркасу фюзеляжу



	Опис
	Номер
	Сторінки
	Примітка

	Типовий ремонт обшивки, дверей, блістерів та аварійних люків
	1201
	1201 - 1216
	Мал 1202, 1203, 1204, 1205

	Типовий ремонт внутрішніх елементів дверей, блістерів та аварійних люків  
	1202
	1217 - 1219
	Мал. 1206

	Типова заміна кабелів, блістерів, дверей та замків на вікнах аварійних люків
	1203
	1220 - 1224
	

	Типовий ремонт силового каркасу фюзеляжу
	1204
	1225 - 1234
	Мал. 1207 - 1211

	Типовий ремонт зовнішньої обшивки та силової установки клеєварної конструкції каркасу
	1205
	1235 - 1236
	

	Типовий ремонт з'єднання шпангоута та поздовжньої балки в місцях пошкодження діаметром 20-40 мм
	1206
	1237 - 1239
	

	Типова заміна підсилювальної накладки, яка встановлена раніше при ремонті пошкоджень
	1207
	1240 - 1241
	Мал. 1212

	Типова заміна обшивки в місцях між сусідніми шпангоутами та поздовжніми елементами жорстокості 
	1208
	1242 - 1243
	

	Типовий ремонт зовнішньої обшивки фюзеляжу, при відсутності доступу для клепки.  Монтаж технічного люку
	1209
	1244 - 1247
	Мал. 1213

	Типовий ремонт елементів герметизації
	1210
	1248 - 1250
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	Мал. 1201 Схема розташування Блістерів, Дверей та Аварійних Люків







Таблиця 1202 –Список Частин до Малюнку 1 – Схема розташування блістерів, дверей та аварійних люків

	Номер
	Опис предмету
	Малюнок №
	Кількість 
	Примітка

	1
	Середня частина фюзеляжу
	8АМТ-0300-00
	1
	(Дов. Секція 053.10.20)

	2
	Ліві зсувні двері
	8АТ-0338-00
	1
	(Дов. Секція 052.10.10)

	3
	Зсувний блістер 
 (Лівий/Правий)
	8АТ-0200-400-1/-2
	2
	(Дов. Секція 052.20.00)

	4
	Праві зсувні двері
	8АТ-0338-1000.973
	1
	(Дов. Секція 052.10.40)

	5
	Вікно аварійного люку
(велике або мале)
	8АМТ-0300-800  (мале)
8АМТ.0385.2000 (велике)
	3

3
	(Дов. Секція 052.20.30)

	6
	Аварійний люк
	8АМТ.0700.100
	1
	(Дов. Секція
052.30.11)

	7
	Вантажна стулка

	8АТ.0700.00
	1 Лівий
2 Правий
	(Дов. Секція 052.30.10)
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