АННОТАЦИЯ
….. И. В. Метод повышения устойчивости радиосвязи подразделений ……. – Рукопись.
Диссертация на соискание научной степени кандидата технических наук по специальности 05.12.13 – радиотехнические устройства и средства телекоммуникаций. - …… национальный университет радиоэлектроники, ….., 2016.
Диссертация посвящена разработке дополнительных средств защиты от преднамеренных помех, моделей радиоканалов и метода определения зон устойчивой радиосвязи подразделений….., которые позволяют повысить устойчивость радиосвязи.
Проведённый анализ состояния связи подразделений …… необходимость повышения устойчивости радиосвязи. Определено, что одним из возможных способов повышения устойчивости радиосвязи является разработка методов эффективного применения дополнительных средств защиты от преднамеренных помех. В работе предложен метод повышения устойчивости радиосвязи подразделений ……., в котором объединены компьютерная модель работы канала радиосвязи в условиях радиоподавления и разработанное дополнительное средство защиты от преднамеренных помех. Использование этого метода позволяет увеличить зону устойчивой радиосвязи в 2,3и 3,71 при использовании в качестве зеркала (отражателя ) в дополнительном средстве защиты от преднамеренных помех  одного  и трех противоядерных алюминиевых щитов соответственно.
Предложена математическая модель канала радиосвязи в условиях радиоподавления на основе принципа суперпозиции при учете действия нескольких средств подавления, пространственных координат взаимного расположения и коэффициентов направленного действия дополнительного средства защиты от преднамеренных помех.
Получена имитационная модель работы канала радиосвязи, которая формализует описание процесса ведения радиоэлектронного обмена в условиях радиоподавления применяя, теорию конечных автоматов Мура и математическую модель канала радиосвязи в условиях радиоподавления. Эта имитационная модель позволяет определить коэффициент подавления в каждой точке пространства и оптимальные азимуты направления дополнительного средства защиты по отношению к источникам преднамеренных помех.
Разработан метод определения зоны устойчивой радиосвязи подразделений ……, который использует численный алгоритм распространения волны и имитационную модели работы канала радиосвязи в условиях радиоподавления. Программная реализация этого метода позволяет получить уточненные значения изолинии и предоставляет всю необходимую исходную информацию для планирования мероприятий радиоэлектронного противодействия.
Полученные в ходе диссертационного исследования результаты подтверждены экспериментами.
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The thesis for the degree of candidate of technical sciences, specialty 05.12.13 - radio engineering devices and telecommunication facilities (technical sciences). - …..National University of Radio Electronics, 2016.
Dissertation is devoted to the development of additional protection means   against jamming, radio channel models and method for determining areas of stable radio communications in units of …… that allows improving the stability of radio communications.
The analysis of communication status in units of the …….  has shown that there is a need for improving the stability of radio communications. It was determined that one of the possible ways to improve the stability of radio communications is the development of methods of efficient implementation of additional protection means against jamming. In this paper we propose a method of improving the stability of radio communications in units of ……  that combines computer model of the radio channel activity under radio suppression conditions and developed additional protection facility against jamming. Using this method allows to expand the area of stable radio communication in  2,3 and  3,71 by using of  one and three antinuclear aluma shields accordingly as  a mirror (reflector) in additional protection facility against jamming.
Mathematical model of the radio channel was offered under the radio suppression conditions on the basis of superposition principle by taking into account actions of a number of suppression devices, space coordinates of mutual disposition and directive gains of the additional protection facility against jamming.
Simulation model of the radio channel activity that formalizes the description of the process for conducting a radio electronic exchange under the radio suppression conditions by applying the finite state machine theory (Moore theory) and mathematical model of the radio channel under the radio suppression conditions became available. This simulation model allows determining the suppression rate in each point of space and the best possible azimuths of additional protection facility in relation to the jamming sources.
Method for determining area of ​​stable radio communications in units of National Guard of Ukraine that uses numerical algorithm of wave-propagation and simulation model of the radio channel activity under the radio suppression conditions was developed. Software implementation of this method allows getting more specific isocurve data ​​and provides all necessary background information for planning of jamming support events.
Results obtained during the thesis research are confirmed by experiments. 
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