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1. GENERAL TECHNICAL PART
             In accordance with the Law of Ukraine "On protection of atmospheric air", "Regulations on state monitoring of the environment" approved by the Cabinet of Ministers of Ukraine №785 of 23.09.93 and "Regulations on state recording in regard to atmospheric air" approved by the Cabinet of Ministers of Ukraine No.1073 of 29.12.93. the employees of  “PROFEKOLOG” LLC namely head of testing laboratory Zviaholska A.V. and laboratory assistant Boiko S.P. 
with occupational safety manager “UKROLIYAPRODUCT” ADDITIONAL RESPONSIBILITY COMPAY Chopenko N.B. an  instrumental inspection was carried out from 
November 15 till November 16, 2016 to detect emission of harmful substances into the atmosphere from controlled stationary emission sources  of “UKROLIYAPRODUCT” ADDITIONAL RESPONSIBILITY COMPAY, at the address: 146, Parkova str., the city of Zinkiv, Poltava oblast, 38100.
            The work carried out in accordance with planned schedule under the work performance/service delivery contract.
            The objective of work performance - harmful substances emission evaluation by direct instrumental measurement for verification of compliance to permit for air pollutant emissions.  
             According to the requirements that are set in permit for air pollutant emissions for UKROLIYAPRODUCT” ADDITIONAL RESPONSIBILITY COMPAY the enterprise, that has established maximum permissible emissions  is obliged to organize control system over the maximum permissible emission compliance that is approved in established order at the enterprise as well as in Local Authorities of  the Ministry of Natural Resources of Ukraine.
            “UKROLIYAPRODUCT” ADDITIONAL RESPONSIBILITY COMPAY requires the control over maximum permissible emission standards compliance directly at emission sources. Control over established standards emission of the pollutants into the environment includes the determination of harmful substances mass per unit of time from the source of contamination and comparison of this index with established standards of maximum permissible emission.
               When performing the control over maximum permissible emission compliance, direct method of measurements should be applied, using measurements of concentration of harmful substances and volume of gas-and-air mixture in areas of direct spot of emission into the atmosphere. When performing the control over maximum permissible emission compliance, emission of harmful substances are determined in a period of 20 min., one-time maximum permissible concentration belongs to. If the period of emission of harmful substances into the atmosphere is less than 20 min., the control is performed during the full time of the emission of the substance into the atmosphere. 
               Control over maximum-permissible emission compliance is performed by the methodic stated in:
1.”Collection of methods on determination of concentration of polluting substances in industrial emissions” L.: Hydrometeoizdat, 1987
2. “Instruction on collection of gas-and-dust streams samples” Ukrainian Research Center of technical ecology, Kyiv, 1993
          According to the classification the following type of control is recommended:
1. By means of determination of the parameter, that is under the control – direct, calculated;
2. At the spot of control  - source of emission, at the limits of C33;
3. At the volume of control – complete, random;
4. By means of measurements that are used – laboratory; 
5. By form of carrying out – scheduled, out-of-schedule.
             The enterprise annually sets the sampling frequency, list of index under control, analysis methodic applied, amount and procedure of information submission on harmful substances emission into the environment (according to the conditions specified in Permit for air pollutant emissions).
[bookmark: _GoBack]                Exact information on maximum-permissible emission standards compliance control for 2016 of             “UKROLIYAPRODUCT” ADDITIONAL RESPONSIBILITY COMPAY, at the address: 146, Parkova str.,  the city of Zinkiv, Poltava oblast, 38100, on each source and ingredient, serial number of sources their origin, substances under the control, regulation value (g/s, mg/m3) specified in the table 3 (table 3  - 
“Control measures on maximum permissible emission standards compliance”).
               Furnishing and maintaining the special control point (gauge hatch, aerodynamic holes etc.) running should be carried out by subdivisions of the enterprise which maintain ventilation and dust-exhaust system.
               In case of excess of the maximum-permissible emissions due to the accident, the enterprise is obliged to inform atmosphere protection authorities and take measures to reduce harmful substances to the atmosphere till the technological equipment and elimination of the consequences of atmosphere pollution as well as inform of the accident and arrange measures.
 

3. CONTROL RESULTS OF MAXIMUM-PERMISSIBLE EMISSION SATANDARDS 
                                 COMPLIANCE IN 2016 AT EMISSION SOURCES

                 Aerodynamic and dust-and-gas measurements at the stationary emission sources are performed in accordance with atmospheric harmful emissions permit of the “UKROLIYAPRODUCT” ADDITIONAL RESPONSIBILITY COMPAY, at the address: 146, Parkova str., the city of Zinkiv, Poltava oblast, 38100. As a result of aerodynamic parameters of the gas-and-air mixture when exit out of the sources had been determined – speed (m/sec), flow rate (m3/sec) and temperature (°C), as well as concentration of the harmful substances in the stream (mg/m3). The obtained values of maximum single emission (g/sec) and concentration of harmful substances determined in the mouth of the sources were compared with permitted values in accordance with permit for air pollutant emissions. 
               As a result of studying of the project of maximum-permissible emissions, the inspection of technological process of the enterprise, inspection of the conformity of the existing operating conditions of the source of the formation and sources of polluting emissions to the operating conditions that are described in the draft of maximum-permissible emissions, visual inspection of the sources of formation and sources of air pollutant emissions, identification of the character of the formation of the pollutant emissions, the following had been established:
· There are no new sources put into service or sources that are put out of service at the industrial site.
· Technical equipment loading (sources of formation of polluting substances), and, accordingly, the loading of sources of the pollutant emissions corresponds to the loading that are introduced in the draft of maximum-permissible levels standards.
· Parameters that influence the condition of air basin, at the sources of polluting emissions have not changed.
· According to the draft of maximum permissible emissions the control over the emissions at the controlled sources should be carried out by means of direct measurements or by calculation method in case when previous method is not possible or inexpedient.
· Control values of intensity of emission of all pollution substances of other sources of formation and sources of emission are obtained by means of calculation method. 
             The results of control measurements and comparison of the amount of harmful substances emitted to the value of permitted emissions are specified in Stationary sources emission sampling REPORT of the present statement.
            CONCLUSION:
            As a result of the control over the maximum-permissible emission standards compliance at stationary sources of “UKROLIYAORDUCT” ADITIONAL RESPONSIILITY COMPANY, at the address: 146, Parkova str., the city of Zinkiv, Poltava oblast, 38100 in year 2016  the excess of standard value of maximum-permissible emissions is not detected.







