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Объект "Укрытие" - объект "Укрытие" представляет собой разрушенный запроектной аварией блок № 4 Чернобыльской АЭС, который утратил все функциональные свойства энергоблока, и на котором выполнены первоочередные мероприятия для уменьшения последствий аварии и продолжаются работы по обеспечению его ядерной и радиационной безопасности.
Опасность - совокупность факторов, сопряженная с эксплуатацией промышленного предприятия постоянно действующая или случайно возникающая в результате некоторого инициирующего события либо при некотором стечении обстоятельств, оказывающих (способных оказать) негативное воздействие на реципиентов.
Радиационная авария - любое незапланированное событие на любом объекте с радиационной или радиационно-ядерной технологией, если при возникновении этого события выполняются два необходимые и достаточные условия:
· потеря контроля над источником ионизирующего излучения;
· реальное (или потенциальное) облучение людей, связанное с утерей контроля над источником ионизирующего излучения.
Несчастный случай – совокупность событий и обстоятельств, повлекшее за собой получение травмы или смерть человека.
Радиационная безопасность - соблюдение допустимых пределов радиационного влияния на персонал, население и окружающую природную среду, установленных нормами, правилами и стандартами по безопасности.
Радиационная защита - совокупность радиационно-гигиенических, проектно-конструкторских, технических и организационных мероприятий, направленных на обеспечение радиационной безопасности.
Радиоактивные отходы - материальные объекты и субстанции, активность радионуклидов или радиоактивное загрязнение которых превышает пределы, установленные действующими нормами, при условии, что использование этих объектов и субстанций не предусматривается.
Риск – вероятность возникновения негативных событий.
Аварийная ситуация – состояние потенциально опасного объекта, характеризующееся нарушением пределов и (или) условий безопасной эксплуатации, но не перешедшее в аварию, при котором все неблагоприятные воздействия источников опасности на персонал, население и окружающую среду удерживаются в приемлемых пределах посредством соответствующих предусмотренных проектом технических средств.
Аварийное состояние – состояние объектов, при котором авария произошла или может произойти.
Аварийный план – план действий в случае возникновения аварии на любом объекте, где осуществляется практическая деятельность, связанная с радиационными или радиационно-ядерными технологиями. 
Запроектная авария – авария, вызванная не учитываемыми для проектных аварий исходными событиями или сопровождающаяся дополнительными, по сравнению с проектными авариями, отказами систем безопасности сверх единичного отказа, либо реализацией ошибочных решений персонала.
НСС – начальник смены Чернобыльской АЭС
[bookmark: _Toc251226532]  ДЕЙСТВИЯ ПЕРСОНАЛА ПРИ ВОЗНИКНОВЕНИИ РАДИАЦИОННОЙ АВАРИИ
Исходными событиями, которые могут привести к радиационной аварии на объекте «Укрытие» могут быть:
Выход радиоактивных веществ и/или ионизирующих излучений за установленные границы;
Пожар в результате молнии, смерча, обрушения конструкций, отказа оборудования, ошибок персонала, работ по ПОМ;
Выход из строя систем управления запроектной аварией;
Обрушение кровли и строительных конструкций в результате деградации конструкционных материалов, в результате землетрясения, смерча или ураганного ветра, пожара, ошибок персонала, отказа оборудования, проведения работ по ПОМ;
Падение кранов и грузов при проведении работ на ОУ;
Обнаружение неизвестных источников ионизирующего излучения при проведении работ на ОУ;
Увеличение уровня грунтовых вод и затопление помещений, содержащих большое количество радиоактивных веществ. Сильный дождь, снег и последующее повышение уровня и скопления воды в помещениях ОУ;
Хищение источников ионизирующего излучения, террористические акты.
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Shelter Object is Unit 4 of Chernobyl NPP destroyed as the result of Beyond Design Basis Accident, which lost all functional properties of power unit, where foremost actions on reducing consequences of accident were undertaken and works on ensuring nuclear and radiation safety continue up to date.
Hazard is a complex of factors associated with operation of industrial enterprise, ongoing or arising accidentally as a result of some initiating event or some concurrence of circumstances, adversely effecting (potentially effecting) the recipients.
Radiation Accident is any unplanned event happened at any facility equipped with radiological and nuclear/radiation technology provided two necessary and sufficient conditions are met:
· loss of control over a source of ionizing radiation;
· actual (or potential) irradiation of people related to loss of control over source of ionizing radiation.
Accident – complex of events and circumstances resulted in injury or death of the person.
Radiation Safety – adherence to permissible limits of radiation impact on the personnel, public and environment established by the safety codes, rules and standards.
Radiation Protection – set of radiological and hygiene, design, technical and organizational measures aimed at ensuring radiation safety.
Radioactive Waste – materials and substances, which radionuclide activity or radioactive contamination exceed the limits established in regulations under the condition that the use of these objects and substances is not provided for.
Risk – probability of negative events occurrence.
Emergency Situation – condition of a potentially hazardous facility characterized by infringement of operational limits and (or) safe operating conditions, which has not passed into accident, and under which all unfavorable impacts of hazard source on the personnel, public and environment are maintained within acceptable limits by means of respective facilities envisaged by the design.
Accident State – state of facilities, wherein the accident has occurred or may occur.
Emergency Plan – plan of actions undertaken in case of accident occurred at any facility, where practical activity related to radiological or radiation/nuclear technologies are carried out. 
Beyond Design Basis Accident – an accident caused by initiating events not taken into account for design bases accident or accomplished by additional safety system failures above and beyond the single failure assumed for design purposes or by faulty personnel decisions.
PSS – Plant Shift Supervisor
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Initiating events that may result in radiation accident at the Shelter Object are as follows:
Release of radioactive substances and/or ionizing radiation over set limits;
Fire caused by lightning, tornado, fall of structures, equipment failures, personnel errors, activities, conducting under SIP;
Failure of prevention management system against the beyond design basis accident;
Fall of roof and engineering structures as a result of construction materials’ degradation due to earthquake, tornado, activities, conducting under SIP;
Fall of cranes and cargo, while conducting works at the Shelter Object;
Reveal of undefined ionizing radiation sources, while conducting works at the SO;
Increase of ground water level and flooding of premises, which contain a great quantity of radioactive substances. Heavy rain and snow cause the following increase of water level and its accumulation in SO premises;
Unauthorized removal of ionizing radiation sources, terrorist attacks.
[bookmark: _GoBack]
