ТЕСТ ПО ОБЩЕТЕХНИЧЕСКОЙ ТЕМАТИКЕ

Английский → Русский

	Cleanliness
It is generally easier to identify problems on clean plant. Dirt can often hide or disguise minor problems so that faults can not be readily identified. For example, dirty sensors or electrical contacts can produce erratic and/or intermittent faults in control equipment, which prevents the plant from operating.
Debris in the boiler house can be a potential fire risk, especially--if it comes into contact with a fuel leak. Keep the area surrounding the combustion equipment and its associated equipment clear of debris, dust and rubbish. If debris is sucked into the air intake of a fan, the fan impeller could be seriously damaged.


	Чистота

Обычно легче обнаружить неисправности на чистом оборудовании. Грязь часто может скрывать или маскировать мелкие неисправности, что затрудняет обнаружение дефектов. Например, загрязненные датчики или электрические контакты могут стать причиной неустойчивых и/или периодически возникающих сбоев в аппаратуре автоматического регулирования, которые препятствуют управлению оборудованием.

Мусор в котельной может создавать потенциальную опасность возгорания, особенно при утечке топлива. Необходимо содержать в чистоте пространство вокруг горелочно-топочного оборудования и сопутствующей аппаратуры, избегая попадания туда мусора и пыли. Если инородные частицы затянет в воздухозаборник вентилятора, рабочее колесо вентилятора может быть серьезно повреждено.


