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Привет, ребята! Меня зовут Дмитриев Станислав. В прошлом семестре я закончил “design studio“ у профессора Liesler. Это “design studio“ занимается, прежде всего, пассивными, активными и экологичными зданиями и функциональным проектированием. По началу, я очень боялся записываться в это “design studio“ потому что оно основывается на методологии и использовании программ, которые я не умею и не знаю.  Активный дом с положительным энергобалансом — это здание, которое получает энергию из окружающей среды с помощью альтернативных источников, в количестве превышающем собственные нужны. Для минимизации энерго потерь и экономии ресурсов применяются лучшие технологии пассивных и умных домов. Но я все-таки решился. Нашим заданием было: Спроектировать активный спортивный клуб с кафе, которое имеет вид на Вышеградский замок. Все это усложнялось и тем, что мы имели определенное количество помещений с определенной минимальной площадью. А так же спортивный зал, размер которого, мы не могли менять. Также солнечные панели, которые мы могли расположить только на крыше, в неограниченном количестве. И, конечно же, наш проект находился на острове, называемый „Cisarska Louka ”, который временами бывает затоплен. Поэтому все без исключения должны были использовать сваи.

Потратив месяц  на изучение специализированной литературы, я приступил к действиям. Каждое активное или пассивное здание имеет простые формы. Идеальное решение-это куб. Это объяснятся тем, что у него очень хорошее соотношение площади поверхности к его объему. Я не очень хотел делать куб, так как в то время я очень сильно был одухотворен простотой и функциональностью японской архитектуры, а так же их подчеркивание горизонтальных форм. Поэтому я решил, что просчет в форме восполню количеством солнечных панелей. Почему нет? Если мы не ограниченны в этом. В течение месяца я проектировал разные диспозиционные планировки, а так же минимальные  размеры санузла, имеющий комфортные интимные душевые, прилегающие к минимальным размерам раздевалок. В конечном итоге мое здание разделилось на две самостоятельно функционирущие части. Первая часть состояла из спортзала, раздевалок, склада и травм. пункта, диагностики. Вторая же имела кафе с санузлами и складом. Великолепно две части делил коридор. А общей частью была терраса с видом на соседний берег реки, где глаз радовала архитектура и наш всеми любимый замок. 

Немалую роль в проектировке играла ориентация здания. Остров был ориентирован длинной осью на северо-юг.  Чехия имеет две разные тепловые зоны, что означает разные тепловые показатели зимой и летом. Также я учитывал, что солнцу встает на востоке и садится на западе. Что зимой солнце ниже, чем летом. Очень долго играя с планировкой, высотой стен, форм окон и их размерами, я пришел к финальному результату. Спортзал у меня был ориентирован на запад. Раздевалки на северо-восток, потому что это единственные общественные помещения, которые имели наименьшие окна. Кафе  было ориентировано на юго-восток, потому что имело самые большие окна. Они также не были простыми. Они были трехслойные, что защищало от утечки тепла и гарантировало сбор энергии зимой.

Отныне моя модель получала больше энергии, чем расходовала. Один не маловажный факт, что структуру стен внутренних и наружных мы не решали. Все использовали heat transfer coefficient, который нам дали, поэтому от части наш проект не был столь тяжелым.  Итоговое здание радовало моих глаз и удовлетворяло условиям проекта. В плане функциональности оно сопоставимо с авангардной архитектурой 20 столетия. Внешний вид имел отголоски пост-модерны, когда функциональность была не единственным качеством здания. Одним из главных композиционных частей моего здания были сваи, которые поддерживали железобетонный фундамент здания, а также защищали от наводнения. Конструкция здания основывалась на s wooden skeleton composed of stanches and beems, it same times called two by four or baume frame systém. Все внутренние перегородки несущие. Здание имеет плоскую крышу, приподнятую в зоне спортзала. А так же  ленточные окна разных размеров. Также на обшивку здания я использовал дерево для придания человечности зданию, а также  цементные плиты. Комбинация этих материалов изящно подчеркивали горизонтальность моего здания.
 
Заключение: Данное “design studio“  дало мне минимальные представления о методологии, о способе как возможно воспринимать архитектуру, какие возможности оно дает и в чем она ограничивает. Спустя 6 месяцев после окончания ательера, я вижу много недочетов в своем проекте, которые я бы не допустил, если бы делал сейчас. Но на то она и учеба, чтобы чередой проб и ошибок чему-то научится. Безусловно, я получил большой багаж знаний, и представление к чему движется европейская архитектура. Ведь стандарты, которые примут в Европе к 2020, будут вынуждать строить здания с минимальной тепловой потерей. До меня пришло осознание того, какие здания и где я хочу строить. Что для меня большой плюс. Я понял, что хочу проектировать здания в южных странах, где я могу проектировать пространства без ограничений в форме. Ведь, метод проектировки несимметричных пространств дает человеку больше эмоциональных и психологических выгод. Я определился, что моим направлением станет проектировка частных домов и вилл.


	Перевод
A job applicant. Presentation

Hey guys! My name is Dmitriyev Stanislav. Passed semester I've accomplished study at "design studio" guided by professor Liesler. This "design studio" is firstly engaged in passive, active and eco-friendly buildings and functional design. At the beginning, I was much scared to enroll to this "design studio" because it is based on methodology and using programs I was not skilled in and I didn’t know. The active house with a positive energy balance is a building to receive its energy from environment by means of alternative sources, in the quantity exceeding own demand. Eliminating power losses and resource saving are ensured by applying the best technologies of passive and smart houses. Finally I ventured to do it. The task we got was to design active sports club with cafe which has a view to the Vyshegradsky castle. All this became complicated by the fact we had a certain number of premises with defining minimal area. And also the gym, which dimension, we couldn’t modify. On top of that, there were solar panels, which we could place solely on a roof in unlimited amount. And of course, our project was located on the island, called "Cisarska Louka", being flooded with times. Therefore all students without exception had to use piles.

Having spent month for studying specialized literature, I took my actions. Each active or passive building has simple forms.  A cube must be an ideal decision. It is explained by the fact that it has very good ratio of surface area to its volume. I didn’t really want to do a cube, as that time I was strongly inspired by simplicity and functionality of Japanese architecture as well as its emphasizing horizontal forms. Therefore I decided that loophole in shape I will fill by the number of solar panels. Why not? If we are not narrowed herein. Within a month I designed different dispositional layouts, including minimal sizes of a bathroom, having comfortable intimate shower adjacent to the minimal sized change-rooms. Finally my building was divided in two independently functioning section. The first part consisted of the gym, change-rooms, storage, emergency and diagnostics stations. The second had cafe with bathrooms and store. Two parts were perfectly carved by a corridor. The shared section was featured by the terrace with view to the opposite river bank, where the architecture and our favorite castle delighted the eye.  

A considerable role in designing was played by positioning of building. The island was oriented by a long axis north-southwards. The Czech Republic has two different thermal zones, what means different thermal indicators in the winter and in the summer. I also took into account, that the sun rises in the east and sets in the west. That in the winter the sun is lower, than in the summer. Playing long with the layout, height of walls, forms of windows and its dimensions, I came to final result. The gym was positioned by me to the west. Change-rooms were directed to the north-east as the only public premises featured by the smallest windows. The cafe was oriented to the south-east due to the biggest windows. They weren’t simple though and consisted of three-layers that protected from a leakage of heat and guaranteed energy accumulation in the winter.

From now on my model received more energy, than consumed. Important to note that we didn’t decide about internal and external structure of the walls. All participants used the given us heat transfer coefficient, therefore our project wasn't partly so tough. The final building pleased my eye and met the project conditions. In respect of functionality it was comparable to vanguard architecture of the 20th century. Outer appearance displayed echoes of the postmodern, when functionality was not the single feature of building. Piles, which supported a reinforced concrete foundation and also protected from the flood, were one of the main composite parts of my building. The structure of the building was based on s wooden skeleton composed of stanches and beems, same times called two by four or baume frame systém. All internal partitions were bearing. The building had a flat roof raised over a gym zone. And also band window varying in rate. For house coat I used wooden siding to reflect some humanity for the entire construction and also add concrete plates. A combination of these materials gracefully put an accent on horizontal position of my building.

Conclusion: This "design studio" has given me the baseline conception of methodology, a way of possibilities to perceive architecture, opportunities it grants and limits it hedges. 6 months after terminating study at the hotelier, I see many defects in my project which I wouldn't allow if performed now. But the learning represents itself a path you advance by series of tests and mistakes. Certainly, I have gained the big bundle of knowledge and impression, where the European architecture moves. Standards, which will be approved in Europe to 2020, force to construct buildings with minimum thermal loss. I have realized, which buildings and where I desire to construct. That is a big advantage for me. I perceived that I want to develop buildings in the southern countries, where I could project spaces without restrictions in shape. Then the method of engineering asymmetrical spaces gives the person more emotional and psychological benefits. I was defined, that projecting private houses and villas will become my stream.



