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This type offers the possibility to add content to the messages without having to extend the message definition (i.e. the definition Excel file), by passing parameters and values as name-value pairs in a generic way. In order to avoid ambiguity, parameter names are always in capital letters (upper case).

	TypeParameterList

	Name
	Comment
	Type

	ParameterName
	Defined name of the parameter.
The name must be agreed between the communication partners.
In order to avoid ambiguity, the parameter name is always in capital letters (upper case).
	string
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This type is used as header in all messages of the L2 interface for both sending and receiving sides.

	TypeHeader

	Name
	Comment
	Type

	TelegramType
	Message identification, for dispatch control, a name which should help understanding the message context (e.g. ProcessStateL22PES, ProcessDataPES2L2 …).
	string

	TelegramLength
	Message length, for quality check including the header and body
	string

	Sender
	Source of message, short name of the Sender
	string

	Receiver
	Destination of message, short name of the Receiver
	string

	TelegramSeqNo
	Unique message identification, normally a sequence number, used for error analysis
	string

	TimeStamp
	Time at which the message was transferred
	3.1 “TypeTimeStamp”

	AckReq
	Request to send back a GeneralAck message.
NEG: Only in case of negative acknowledge (message handling failed). That is recommended as best practice.
ALW: Always.
NEV: Never, even in case of negative acknowledge.
	string

	ReqTelegramSeqNo
	Sequential number (TypeHeader.TelegramSeqNo) of the message to which this message is responding
	string

	LineId
	For future use. Line identification
	string


1.1  Tип Список параметров
Этот тип позволяет добавлять контент в сообщения без необходимости расширять определение mes-sage (то есть файл Excel определения), передавая параметры и значения в виде пар имя-значение общим способом. Чтобы избежать двусмысленности, имена параметров всегда имеют заглавные буквы (верхний регистр).
	Тип Список параметров

	Имя
	Комментарии 
	Tип

	Имя Параметра
	Определенное имя параметра.
Имя должно быть согласовано между партнерами по коммуникации.
Чтобы избежать двусмысленности, имя параметра всегда имеет заглавные буквы (в верхнем регистре).
	строка



2.2 Тип  заголовок 
Этот тип используется как заголовок во всех сообщениях интерфейса L2 для сторон отправки и приема
	Tип Заголовок 

	Имя
	Комментарии 
	Tип

	Тип Телеграмма 
	Идентификация сообщения, для диспетчеризации, имя, которое должно помочь понять контекст сообщения (например, состояние процессаL22PES, Process DataPES2L2 ...).
	строка

	Длина Телеграммы 
	Длина сообщения, для проверки качества, включая заголовок и корпус
	строка

	Отправитель
	Источник сообщения, короткое имя Отправителя
	строка

	Получатель
	Назначение сообщения, короткое имя получателя
	строка

	Порядковый номер Телеграммы 
	Уникальная идентификация сообщения, обычно порядковый номер, используемый для анализа ошибок
	строка

	Время создания файла 
	Время передачи сообщения
	3.1” Тип Время создания файла”

	Запрос подтверждение приёма сообщения 
	Запрос на отправку сообщения GeneralAck.
NEG: Только в случае отрицательного подтверждения (обработка сообщений не удалась). Это рекомендуется в качестве наилучшей практики.
ALW: Всегда.
NEV: Никогда, даже в случае отрицательного признания.
	строка
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