Electric Kettle User Manual
Thank you for purchasing this electric kettle. Please read this instruction manual carefully before using the appliance for the first time. Proper use and maintenance will ensure safe operation and extend the lifespan of the product.

Safety Instructions
Before connecting the kettle to the power supply, check that the voltage shown on the product label corresponds to your local electrical voltage. Always use the appliance with a grounded electrical outlet.
Do not use the kettle outdoors or in humid environments. Keep the appliance away from direct sunlight, hot surfaces, curtains, and flammable materials. The kettle should only be used for boiling water. Do not use it to heat milk, soup, or other liquids.
Children should use the appliance only under adult supervision. Do not allow children to play with the kettle or the power cord. The surface of the kettle may become hot during operation, so always use the handle provided.

Before First Use
Remove all packaging materials and protective films from the appliance. Wash the inside of the kettle with clean water before first use. Fill the kettle with water to the maximum level mark, boil the water, and pour it out. Repeat this process two or three times to remove any manufacturing residues.

Operating Instructions
Place the kettle on a flat, stable, and dry surface. Open the lid and fill the kettle with clean drinking water. Make sure that the water level is between the minimum and maximum marks indicated inside the appliance.
Close the lid securely before turning the kettle on. Place the kettle onto the base correctly and plug the power cord into the electrical outlet. Press the power switch downward to start boiling water. The indicator light will turn on to show that the appliance is operating.
Do not remove the kettle from the base while it is boiling. Avoid opening the lid during operation because hot steam may cause serious burns. When the water reaches boiling temperature, the kettle will switch off automatically.

Cleaning and Maintenance
Always unplug the appliance and allow it to cool completely before cleaning. Never immerse the kettle, power cord, or base in water or any other liquid.
Use a soft damp cloth to clean the exterior surface. Do not use abrasive cleaners, metal brushes, or chemical products, as they may damage the appliance.
To remove limescale, fill the kettle with a mixture of water and vinegar. Leave the solution inside for approximately one hour, then boil it and rinse the kettle several times with clean water.

Storage Instructions
Store the kettle in a cool and dry place. Ensure that the appliance is unplugged before storage. Wrap the power cord loosely around the base if necessary.

Troubleshooting
If the kettle does not switch on, check whether it is properly connected to the power outlet. If the appliance switches off before boiling, there may be excessive limescale buildup inside the kettle.
If the power cord or appliance becomes damaged, stop using it immediately and contact an authorized service center for repair. Do not attempt to repair the appliance yourself.
